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1 Purpose
1.01 The purpose of this document is to describe the procedure for testing the Corded Swing Machines.
2 Scope 
2.01 This SOP applies to all equipment assembly team members.  The process applies to the following machine ID’s:
E12801EQM0600BA1000 – Basic Sand Dragon, 20”
E012801EQM0607BE1200 – Crewman ORB 20
E012801EQM0607BA1200 – Basic Sand Dragon 20, Canadian
E012801EQM0607BE1200 – Crewman ORB 20, Canadian
E012806EQM0600BA1000 – Basic Sand Dragon, 20”, w/ Weights
E012806EQM0600BE1200 – Crewman ORB 20, w/Weights
E012806EQM0607BA1200 – Basic Sand Dragon 20, w/Weights, Canadian
E012806EQM0600BE1200 – Crewman ORB 20, w/Weights, Canadian
E012811EQM0600BA1000 – Basic Sand Dragon, 28”, w/Weights
E012811EQM0600BE1000 – Crewman 28 ORB, w/Weights
E012811EQM0607BA1200 – Basic Sand Dragon 28, w/Weights, Canadian
E012811EQM0607BE1200 – Crewman ORB 28, w/Weights Canadian

3 Responsibilities
3.01 The operations manager/supervisor is responsible for enforcing this SOP.
4 Materials 
4.01 The proper materials needed for this process are listed on the machine work order.
4.02 Load Tester / Hi-Pot Tester
5 Definitions
5.01 
6 Procedure 
6.01 Lock the machine handle in a suitable operating position.
6.02 Turn on the hi-pot test unit.  Plug the machine into the outlet that goes to the tester.
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6.03 Press the green test button on the hi-pot tester.  The unit will make a chirping sound.  If a buzzer sounds, the machine is wired improperly and should be fixed.  As long as the buzzer does not sound, the machine is ok.
6.04 Plug the machine into an outlet.  Hook the electrical meter up to it so that amp draw can be measured. Note: The machines should be below 15 amps. 
6.05 Operate the machine and make note of the amp draw displayed on the meter.  Verify that the machine will also start and operate by using one hand.  A new switch may need to be used if this condition is not met.
6.06 [bookmark: _Hlk159994227][image: A close-up of a blue box

Description automatically generated][image: A screenshot of a computer

Description automatically generated]Next log into computer and click on Corded Equipment at the top of the page. Record the date, Machine ID, Serial Number, Amperage and pass or fail for Hipot Test. Note: If a failure occurs take a picture and upload into forms. 

6.07 Unplug the machine, raise the handle into the transport position, and place a serial number sticker (81180) onto the back of the handle.  
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6.08 [bookmark: _Hlk159994607]Place a manual, a warranty card, and a tech service card into a plastic bag.  Put the bag with the machine. Reference EQ ID for pad or insert.
6.09 The machine is now ready to be boxed.


7 References (optional section as needed)

8 Training Guide

	Functional Training Groups Requiring Training

	Equipment Assembly Group

	



9 SOP Change Control

	Date of Change
	Reason for Change

	Rev 01 - 4/28/2015
	This is the first version of the S.O.P. hence there are no revisions to this document.

	Rev 02 - 1/16/2018
	Added the Responsibilities Section

	Rev 03 - 2/26/2024
	Changed recording in book to forms and instructions to completed Forms. 

	Rev 04 - 3/6/2025
	Updated Machine ID’s and removed work center note
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