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1. Take 2 wheels (88658) and place 2 bearings (88626) into each wheel (4 total bearings).  The bearings can be placed into the grooves by hand.  There is one on each side of the wheel.
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2. Insert one of the wheels onto the axle (88657) as shown.  Some of the bearings will slide right onto the shaft.  Some of them may need to be pressed on.  If so, use one of the insertion tools to place the bearings at the needed distance from the end of the shaft.
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3. Slide the inner wheel spacer (88661) onto the middle of the shaft.
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4. Install the second wheel onto the other end of the axle.  If the bearings need to be pressed on, use the other insertion tool provided.  This will place the bearings at the necessary distance from the end of the shaft.
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5. Place the right wheel spacer (88659) onto the longer exposed end of the axle.  Then place a washer (82773) onto each end of the shaft.
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