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Initial:

1. Start with a solution valve (88589).  The valve will come with a black knob.  Discard the knob.
2. Use thread sealant on all threaded connections.  Make not of the solution flow direction.  There is an arrow on the valve body.  Thread the barbed elbow (88590) into the inlet side of the valve.  Then thread a barbed straight fitting (88591) into the exit side of the valve.  Note the orientation of the fittings.

[image: image2.jpg][image: image1.png]Windows Photo Viewer

403PM
11/28/2012

Desitop B+ vy 43




Flow Direction





Straight





Elbow





Valve








STANDARD OPERATING PROCEDURE - CONFIDENTIAL

Page 2 of 2

