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1. Take a machine cover (88679) and install 2 gaskets (88703) around the vacuum ports. 
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2. Nex bolt the side splash guard in place.  This step requires a splash guard (88742), a band clamp (88743), a nut plate (88745), and 3 screws (88746).  The splash guard and the band clamp go on the outside of the cover while the nut plate goes on the inside of the cover.
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3. Place a flow control decal (89601) on the outside of the cover around the hole where the solution control knob will go.
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