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1. Install 2 o-rings (88606) onto the plunger (88699) as shown in the photo.  There is a groove in the plunger for each o-ring.  Place a small amount of silicone lubricant onto the o-rings once installed.
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2. Place a female coupling (88610) onto the table with the flange side up.  Then insert the plunger with the o-rings into the coupling in the orientation shown.
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3. Take a solution tank (88675) and clean out any shaving or debris from the inside.  You may need to use a vaccum.  Place the tank upside down on the table and put a bead of sealant around the opening in the bottom of the tank.  Run the beam right over the 6 screw holes that surround the central opening.
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4. Place a plunger spring into the center of the opening.
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5. Place the female coupling with the plunger onto the solution tank.  Verify that the spring lines up with the plunger.  Attach the coupling to the tank using 6 screws (88705) and 6 washers (20292).  It is best to get a few screws started before completely tightening them down.  Verify that the sealant spreads out and gives good coverage over the entire flange of the coupling.  This will help ensure that the tank does not leak.  Flip the tank over and look into the top opening.  Check to see that the sealant is not blocking any of the holes in the bottom of the tank.  This will ensure adequate solution flow.  Allow the sealant to cure overnight before putting any water in the tank.
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6. On the side of the solution tank is a groove for the sight glass.  There is a hole on both the top and bottom of the tank.  Install a grommet (88717) into each hole.  You may need to use a small flathead screwdriver to get the grommet started into the hole.  Be careful not to damage the grommet during this step.
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7. Tank the grommet insertion tool and make sure that the grommet is installed completely.  Place the stud on the tool into the grommet until the shoulder bottoms out on the flange.  Use a mallet and tap the back end of the tool to verify that the grommet is fluch with the tank.
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8. Take 8 ¼” of clear plastic tubing (88689) and press a barbed elbow fitting (88739) into each end of it.  Then take a mallet and gently tap the barbed fittings into the grommets on the tank.  Do not hit the fittings too hard as they can break.  Note: Putting a little dish soap on the barbed fittings allows for easier installation.
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9. Now the solution tank lid needs to be assembled.  Take a solution tank cap (88677) and verify that the hole in it is 11mm in diameter.  If it is not, drill it out to the proper size.  The vent pin will not operate properly if this hole is not correct.
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10. Place a vent pin (88709) into the hole in the cap in the orientation shown.
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11. An o-ring now needs to be placed onto the vent pin.  The groove for the o-ring is about ½ way down the pin.  Start by placing the o-ring (88710) over the end of the pin.  Slide the o-ring down the shaft until it gets down into the cap.  At this point, use a small flathead screwdriver to finish pushing the o-ring into the groove.  Push the o-ring down little by little and working around the pin.  Be careful not to cut it.
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12. Place a gasket (88711) over the outer ring of the cap.
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13. Attach an e-clip (88712) in the groove at the bottom of the vent pin.  The easiest way to install it is by using a pair of channel locks as shown below.
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14. With the cap fully assembled.  Pull the pin upward to verify that o-ring seals.  The pin should stay in the up position.  Fix any issues.  Install the cap assembly onto the solution tank.
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15. Install the solution tank handle (88704) to the tank using 4 screws (88802).  The best method is to start threading the outer two screws before completely tightening either one.  This lines the handle up.
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