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1. Start with a solution pump (85553).  On the top of the solution pump body near the Warning label, cut off the extra plastic extrusion as shown below.  The photo below shows the extrusion removed.
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2. Next assemble the brass fittings to the pump.  Use thread sealant on all threaded connections.  Thread a brass barbed elbow (88588) into the inlet port of the pump.  Next thread a brass T-fitting (88670) into the outlet port of the pump.  Into the end of the T-fitting, thread a straight barbed fitting (88669).  Thread another brass elbow (88588) into the remaining port of the T-fitting.  Note the orientation of all of the fittings below.
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