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1. The solution filter assembly consists of an inline filter (88595), two pieces of braided hose (EP50155 which is 5.5” long and EP50156 which is 8.5” long), and 2 clamps (89540).
2. The filter has an arrow on it that indicated the direction of flow through it.  Locate this arrow before assembly.  Place the shorter piece of hose (EP50155) on the “upstream” side of the filter and the longer piece of hose (EP50156) on the “downstream” side of the filter.  The hoses simply press onto the ends of the filter.
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3. Once the hoses are in place, install the clamps on each end of the filter using the pinch tool.
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