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1. Take a transport wheel axle (88630) and pound an axle cap (83143) onto one end using the installation tool.  Place the cap into the pocket on the tool and pound it on with a hammer.
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2. Insert 2 wheels (81125), 2 nylon washers (83145), and 2 spring washers (83269) onto the axle in the order shown below.  Pound another axle cap onto the other side of the axle.
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