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1. Take a foot pedal weldment (88647) and clean out the 15mm hole using a reamer.  Occasionally, burrs will be in this hole making it difficult to install the bushing.
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2. Place a bushing (88643) into the hole.  Be sure to install it in the orientation shown.
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3. Place a torsion spring (88623) around the head of the bushing.  Next, place the foot pedal latch weldment (88652) into position as shown.  Note the orientation of the spring and the foot pedal in the following pictures.  The hooks on the sprint wrap over each of the two weldments.
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4. Place a washer (82773) over the end of the pin on the foot pedal latch weldment.
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5. Install a snap ring into the groove on the end of the pin.  This will hold the pedal in place.  Verify that the snap ring is completely in the groove when complete.
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6. Assemble the remaining two linkage pieces as shown in the photo.  Use a foot pedal link weldment (88654) and a pivot lever linkage left weldment (88653).
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7. Place a washer (82773) over each of the two pins on the link weldment.  Then, install a snap ring (88628) into the groove on each pin.  Ensure the snap rings are completely in the grooves.
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8. Thread 6 set screws (88649) into each of the holes on the end of the linkage.  Just thread them in a little ways as they will be tightened down at another point.
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Pivot Lever Weldment


Link Weldment
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