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1. Bolt the male coupling (88605) to the handle mounting plate weldment (88607).  Place two shims (1 each of 88812 and 88813) between the coupling and weldment.  These shims can be taken out later if there is a solution flow issue with the machine.
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2. Bolt everything together with 4 bolts (83881), 4 washers (83879), and 4 nuts (82256).
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3. Install 2 o-rings (88606) into the grooves on the coupling.
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4. Now the filter assembly needs to be installed.  Reference the “Solution Filter Assembly” SOP for instructions on how to put it together.  First place a clamp (88912) over the shorter piece of hose (EP50155).
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5. Insert the end of the shorter hose (EP50155) over the hose barb on the bottom of the male coupling.  Once fully inserted, slide the clamp down so that it clamps on the barb.
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