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1. Hand assemble the foot pedal link weldment (88654), the pivot lever linkage right weldment (88662), and the right lift arm weldment (88663) as shown below.
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2. Attach all three pieces together using 2 washers (82773) and 2 snap rings (88628).  Ensure the snap ring is properly seated in the groove.
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3. Thread 6 set screws (88649) into the proper holes.  These will be tightened at another time.
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