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1. Start with a lower base (88597).  Place the base upside down on the table.  The three holes shown in the photo below need to be drilled out using a .235” diameter drill bit.  These holes are located on the back side of the base.
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2. Flip the base back over to the top side.  There are 3 holes at the back of the base that need drilled out to the same .235” diameter.
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3. On the front of the base are the last two holes that need drilled out to the same 0.235” diameter.
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4. There are 13 posts on the top side of the base that need to be drilled.  Use a 17/64” drill bit to do this.  Do not force the drill down and be sure to hold it steady to prevent the posts from breaking.
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5. Use the insert insertion tool to screw a brass insert (89563) into each of the 13 posts.  Orient the inserts so that the end with the notch will be inserted first.  Thread the insert onto the tool.
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6. Chuck the insert into a drill and thread the insert into the post until the shoulder on the tool bottoms out on the posts.  Do this step slowly and without too much torque.  If care is not taken, the post can break during this step.  Once the insert is completely threaded in, put the drill in reverse to back the tool out.  The insert should remain in the post.  If it begins to thread out, screw it back in and re-try.
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7. Repeat for the remaining posts.
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Put notch on this end
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