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1. Place a serial number sticker (81180) onto the machine.  The sticker goes on the machine base on the back side of the machine, just under the handle tower weldment.
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2. Put a machine insert (88906) into the bottom of a shipping box (88660).  Make sure the insert sits flat on the bottom.
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3. Place the machine into the shipping box.  Verify that the machine is sitting properly on the insert.
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4. The machine will need a manual packet to go with it.  If the machine is a Betco machine (Genesys), it will need a manual, a Betco warranty registration card, and a tech service business card.  If the machine is a Basic machine (Dirt Dragon, Stanley Steemer, Servicemaster), it will need a manual and a Basic warranty registration card.
5. Turn on the foam packing machine.  All of the foam bags used in the packaging are numbered.  The bags must be put into the box quickly as the foam will expand rather rapidly.  The diagrams below show the locations of the bags for each machine.  Be sure to place a cord  (88683) into each box.  DO NOT FORGET THIS PIECE!!

Betco Machine (Genesys)

-Try to have the foam bags go under the machine slightly.


-The bags have slots on the top, so be careful not to have any foam come out of them.
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Basic Machine (Dirt Dragon, Stanley Steemer, Servicemaster)

-Try to have the foam bags go under the machine slightly.


-The bags have slots on the top, so be careful not to have any foam come out of them.

-Close the flaps of the box for a few seconds when bag #5 is put in.  The foam will fit to the top of the closed box.
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6. Tape the box closed and put onto a pallet for shipment.  Be sure to put a machine ID tag onto each box.  Write the machine serial number on each one.
[image: image8.png]156 PM
2472013

Desitop B+ vy 43




This supports the area around the vac motor





The back of the machine base sits on this step
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