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1 Purpose
1.01 The purpose of this document is to describe the procedure for assembling the Recovery Tank on the Genesys Machine.
2 Scope 
2.01 This SOP applies to all equipment assembly team members.  The process applies to the following machine ID’s:
EP50328EQS0600BE1200 – Recovery Tank Assembly (MSAS)
EP50290EQS0600BE1200 – Recovery Tank Assembly (G20)
3 Responsibilities
3.01 The operations manager/supervisor is responsible for enforcing this SOP.
4 Materials 
4.01 The proper materials needed for this process are listed on the machine work order.
5 Definitions
5.01 
6 Procedure
6.01 Start with a recovery tank (E28575 – MSAS / E28886 – G20).
6.02 Tap out the hole where the lid mounts using a 1 ½” tap. Align tap with hole slowly thread tap through the hole. When tap is in halfway back the tap off making sure it is level. 
6.03 Take a PVC tube (E29577) and but it into a 4” piece. Verify there are no obstructions inside the tank (Note: if obstruction is present grind out the area impeding the tube from being placed). Press the tube into a barbed fitting (E29531).  Thread the fitting into the appropriate location on the recovery tank. 
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6.04 Take a float ball cage mount (E29562) and stick a gasket (E28607) onto the bottom side.  Attach the mount to the tank using 2 hex bolts (E81089) and 2 washers (E28622).
[image: ]Gasket goes between tank and Mount

6.05 Put a float ball shut off (E29563) onto the end of the mount.  Verify float balls are present. Attach it with a clamp (E28990).  Position interlocked portion of the clamp under the gooseneck.
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6.06 Place the vac assembly (Refer to SOP 107 for assembly instructions) into the pocket on the tank.  -On the MSAS, place 3 spacers (E28850) between the bracket and the tank.  Then use 3 washers (E28622) and 3 hex bolts (E81072) to attach the bracket.  
-On the G20, attach the vac bracket with 3 washers (E28622) and 3 hex bolts (E81072).
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6.07 Attach each of the 2 hinges (E28596) to the tank using 4 total flange bolts (E29569).  Slide the hinges towards the back of the tank as shown.
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7 References (optional section as needed)
7.01 
8 Training Guide

	Functional Training Groups Requiring Training

	Equipment Assembly Group

	



9 SOP Change Control

	Date of Change
	Reason for Change

	TBD
	This is the first version of the S.O.P. hence there are no revisions to this document.

	8/9/2021
	Remove the vac motor assembly portion.  That is now its own SOP

	11/2/2023
	Updated steps for current process.

	3/31/2025
	Combined MSAS and G20 instructions.
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