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1 Purpose
1.01 The purpose of this document is to describe the procedure for drilling the dimple into the shaft of the down pressure switch.
2 Scope 
2.01 This SOP applies to all equipment assembly team members.  The process applies to the following machine ID’s:
EP50317EQS0600BE1200 – Standard Controls/BDI Assembly
EP50318EQS0600BE1200 – Standard Controls/Bluetooth BDI Assembly

3 Responsibilities
3.01 The operations manager/supervisor is responsible for enforcing this SOP.
4 Materials 
4.01 Drill press
5 Definitions
5.01 
6 Procedure
6.01 Locate the sample switch.  Place it into the drill fixture as shown.  Use this to set the location of the fixture and the depth of the drill point.  Use a 1/8” drill bit.  Set the stop collar on the press.
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6.02 Once it is set.  Clamp the fixture down and set the collar on the drill for the depth. 
6.03 Drill out the appropriate number of the switches.
[image: ]
7 References (optional section as needed)
7.01 
8 Training Guide

	Functional Training Groups Requiring Training

	Equipment Assembly Group

	



9 SOP Change Control

	Date of Change
	Reason for Change

	Rev 01 
	This is the first version of the S.O.P. hence there are no revisions to this document.

	Rev 02 - 4/2/2025
	Combined MSAS and G20 instructions.
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