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1 Purpose
1.01 The purpose of this document is to describe the procedure for final assembly on the Genesys Mid-Sized Scrubber, Disk Version with Lithium Batteries.
2 Scope 
2.01 This SOP applies to all equipment assembly team members.  The process applies to all machine ID’s:
3 Responsibilities
3.01 The operations manager/supervisor is responsible for enforcing this SOP.
4 Materials 
4.01 The proper materials needed for this process are listed on the machine work order.
5 Definitions
5.01 
6 Procedure
6.01 Place a frame and solution tank assembly (Roller) onto a build cart.
6.02 Place a foam battery spacer (E28785) into place.  Position it so that it is about 1” below tank edge.  
6.03 Install a lithium battery (E28495 for a 200AH battery / E28494 for a 150AH Battery) into the compartment in the orientation shown.
6.04 Place another spacer (E28785) in front of the battery.
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6.05 Attach the end of the squeegee lift cable to the pivot.  Thread a hex nut (E29565) up towards the top of the stud.  Place a flat washer (E28617) over the threaded end and feed the stud through the hole on the squeegee mounting bracket.  Then place a spherical washer (E28717) over the end of the stud and attach everything using another flat washer (E28617) and nut (E29565).  Thread the nut up enough so that the assembly can still pivot properly.
[image: ] [image: ]

6.06 [bookmark: _Hlk120784196]Take an Inner Electrical Panel (E28963).  Add red loctite onto the standoff threads.

[image: A picture containing indoor

Description automatically generated]
6.07 Attach an electrical standoff (E28950) to each stud and snug it in place.  Be careful to not overtighten.  Put some red Loctite onto a set screw (E29447) and thread it into the standoff.  Repeat for the other standoff.

[image: ]

6.08 Mount the inner panel assembly to the solution tank using 2 screws (E28648) and 2 toothed washers (E29446).  It will only fit in one direction as shown.
[image: ]

6.09 Pull the main wire harness back out of the back of the machine, then feed the portion of the main wiring harness that goes to the vac motor into the battery compartment as shown.

[image: ] [image: ]

6.010 Take a set of battery cables (E28497) and separate the two halves.  Note that one half has an inline 100 amp fuse.
[image: ]  [image: ]


6.011 Take the cable set with the fuse and place the positive and negative wires onto the standoffs in the electrical panel.  Place them onto the locations shown.  The Anderson end of the cable should remain in the battery compartment.
[image: ] [image: ]

6.012 Attach the + and – terminals from the main harness to the appropriate standoffs on the panel.  Fan the terminals out so that they tighten up properly.  Unless there are options on the machine, the nuts on the studs can be tightened.  Use a nut (E28853) and a washer (E28617) on each one.  Use a torque wrench to tighten to 8 ft-lbs.  Tug on the wires to ensure they do not move.  When using the torque wrench, only hold on the handle as shown to get an accurate reading. 

[image: ] [image: ]

6.013 Mount the relays from the main harness to the appropriate studs on the panel with hex nuts (E29366).  Ensure they are tight.  The smaller relay goes on top.

[image: ]

6.014 Connect the appropriate connectors on the main harness to a Contactor (E28924).  The hardware is already on the contactor.  There are 2 contactors on the disk machine.  The order of the wires in not critical but to be consistent, place the yellow on top as shown.  Use a ratchet/nut driver to ensure the nuts are fully tightened.  Mount the contactor to the panel using 2 nuts (E28618).  Pull on the wires to make sure they don’t move.
Wire Numbers

[image: ] [image: ] [image: ]12&12/82A
4A&4B
2E
2F
22&22/82
31
4&4A
33

6.015 Connect the appropriate connectors on the main harness to the I-Drive (E28949).  There are 4 single wires, a 2 pin connector, and a 14 pin connector.  Note the labels and locations below.
[image: ]2 pin connector with single brown wire
14 pin connector 
42
10D
52
70

6.016 Attach the I-Drive to the panel using 2 Pan Head Screws (E29382).
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6.017 Feed the wires for the handle console/bail through the holes and into the upper cavity.  
[image: ] [image: ]These 2 wires always stay in the lower compartment

6.018 Take a bail assembly (See the appropriate SOP for assembly instructions) and connect the microswitches to the appropriate wires from the main harness up in the handle attach area of the tank.  The photo shows the correct sequence.  Wire numbers are noted in the photo.
[image: ]8
63A
62
63&63A

6.019 Attach the bail assembly to the solution tank using 2 bolts (E81089) and 2 washers (E81062).  Ensure the wires are coming out of the appropriate side of the bracket as shown.

[image: ]

6.020 Get a handle assembly.  See the appropriate SOP for assembly instructions.  Connect the potentiometer from the handle to the appropriate terminal on the main harness.
[image: ]
6.021 Fasten the plastic handle to the tank using 3 bolts (E81089) and 3 washers (E81062).  Use Blue Loctite on the bolts.  Make sure to not pinch any of the wires on the harness.

[image: ]

6.022 Take an appropriate console panel for lithium (See SOP for Assembly Instructions).
6.023 Connect the 8-pin connector from the main harness to a jumper assembly (E28498).  
[image: ]    [image: ]


6.024 Connect the two wires from the jumper to the two terminals on the back of the hour meter on the console.  It does not matter which wire goes to which terminal.

[image: ]

6.025 If the machine is equipped with SoliChem, connect the two wires from the Solichem LED on the console to the main harness.  These connectors are error proofed.  The wire numbers from the harness are shown.
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6.026 Connect the appropriate wires from the main harness to the down pressure switch.  See the photo for the wiring sequence.
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6.027 Feed the extra wire from the battery meter down through the electrical panel and into the battery compartment.

[image: ]
6.028 Mount the console panel to the handle using 4 screws (E29334).  Tighten by hand and be sure not to overtighten.  Pull on the knob to make sure the panel doesn’t move.  

[image: ]

6.029 Get an outer electrical panel (Refer to the appropriate SOP for assembly instructions).  The lithium version of the panel does not have an on-board charger on it.
6.030 Connect the appropriate connectors from the main harness to the circuit breakers on the panel.  An orbital machine will only have 3 breakers. There are 4 pairs of 2 wires for a disc machine.  The lengths and/or how they are held by the wire ties should give the order.  If not, use the wire numbers shown below.  Right or left terminal does not matter.  If wires 22 & 22A seem too short, cut the zip tie that holds them.  This should give them enough slack to connect.
[image: ]21 & 42
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6.031 If the machine has SoliChem, connect the appropriate connectors from the main harness to the TDS Switch.  It does not matter which switch goes to which terminal.

[image: ]65 & 65A


6.032 Connect the Key Switch to the main harness.  It does not matter which wire goes to which terminal.
[image: ]5/15/57
57



6.033 Connect the solution potentiometer to the appropriate connector on the main harness.  It is a 2 pin connector.
[image: ]23
10R

6.034 Connect the appropriate connectors from the main harness to the control board.  There are 3 terminal blocks to plug in (12 pin, 10 pin, and a 4 pin).

[image: ]

6.035 Connect the pad release button to the appropriate connectors on the main harness.  It does not matter which terminal goes to which wire.
[image: ]29
10C

6.036 Locate the charger interrupt plug on the main wire harness.  It is a connector with purple wires 57 and 57A.   Plug a charger interlock bypass jumper (E28499) into the connector. 

[image: ] [image: ]

6.037 If the Wet Battery Protection Option is needed.  Refer to section 6.01 in SOP EQ 111 (Genesys MSS Final Assembly Options).

6.038 Mount the panel to the tank using 4 washers (E28617) and 4 screws (E28648).  Be careful as they can strip.  Make sure all wires are tucked inside on the cavity and don’t get pinched.  The main portion of the harness should pass through the cutout in the panel.

[image: ]Main Harness should pass through here


6.039 Since this is a lithium unit and doesn’t have an on-board charger, you can remove the cord wrap on the side of the solution tank.  The wrap and the screws can go back into stock.

[image: ]  [image: ]

6.040 Mount the appropriate sized squeegee assembly to the machine.  See the required SOP for assembly instructions.  (35” squeegee for a 26” machine / 40” squeegee for a 28” machine / 45” squeegee for a 32” machine).  Mounting the squeegee will also help keep it from rolling.  

[image: ]

6.041 Ensure the key is in the “OFF” position.  Connect the other end of the battery cable assembly (E28497) to the + and – terminals of the battery.  

[image: ]  [image: ]


6.042 Connect the cable that comes from the battery indicator to the CAN port on the battery.

[image: ]

6.043 Attach the roller track bracket to the solution tank using 4 hex bolts (E81089) and 4 flat washers (E28622).  Use blue Loctite on the threads.  The plate can be allowed to hang low on the slots.

[image: ]

6.044 Place the appropriate sized scrub deck onto the table in front of the machine.  Refer to the proper SOP for scrub deck assembly instructions.  Feed the solution hose and the wire harness coming from the frame through the area shown.

[image: ]

6.045 Take a 1” roller (E28663) and install a roller bushing (E28664) into it.

[image: ]

6.046 Take a clevis pin (E28783) and place a washer (E28622) and a spring (E29328) over it.

[image: ]

6.047 Line the roller bracket on the head with the roller track bracket on the tank.  Place the roller between the uprights on the roller bracket and in line with the holes.  Insert the pin through the bracket and the roller.  Compress the spring to expose the end of the pin and install a washer (E28622) and a cotter pin (E28671) to secure it.

[image: ] [image: ]
[image: ]
6.048 Attach the disk head assembly to the lower frame using 2 clevis pins (E28697) and 2 cotter pins (E28671).  This connects the frame arms to the disk head brackets.
[image: ] [image: ]
6.049 Gently tighten the 3 bolts that hold the roller track bracket in place.  Then tighten the carriage bolt on the end.

[image: ]  [image: ]






6.050 Get a y-fitting (E28747) and see where it will sit based on the current solution hose lengths.  There may be extra hose that can be trimmed.  Position this so that the fitting sits centered above the bracket.  Trim to hoses so that there is no stress on the fitting from the bracket but not so long that it will sag.  Ensure there are no kinks where the hose goes into the deck.

[image: ]Hoses are not stressed against the bracket edges
Centered on bracket


6.051 Plug the brush motors into the appropriate harness terminals.  Note the right and left wires.  The connector with the yellow tape goes to the motor on the assemblers right side (Operators left) (Wires 12A and 10H).
6.052 Use a zip tie (E88890) to bundle the wires and hoses as shown.  Note that the wire for the motor on the operators right side is folded over.  Trim the zip tie when tight.

[image: ] [image: ]

6.053 Get a head lift assembly equipped and a head lift support bracket (E20702).  (Refer to the appropriate SOP for head lift assembly instructions) Insert the support bracket into the bracket as shown.  The slotted holes in the bracket will align with the ones on the head lift.

[image: A metal piece of metal

AI-generated content may be incorrect.]  [image: A hand holding a metal box

AI-generated content may be incorrect.]  
[image: A hand holding a metal box

AI-generated content may be incorrect.]  [image: A metal box with wires and a hand holding a metal pole

AI-generated content may be incorrect.]















6.054 Attach it to the solution tank using 4 bolts (E81089) and 4 washers (E28622).  Use blue Loctite on the bolts.  Tighten them all evenly so that the assembly locates properly against the tank.

[image: A close-up of a machine

Description automatically generated with medium confidence] 

[bookmark: _Hlk150926769]*Note:  Slide head lift support bracket as flush to the tank as possible to minimize the gap between the bracket and tank.
[image: A picture containing red, indoor, engine

Description automatically generated]

6.055 [image: A picture containing person, red

Description automatically generated]Add a red support strap (E20703) above the front fill port.  Attach the support strap using 2 bolts (E10112), 4 washers (E081062) and 2 nuts (E28623) using a ½” wrench.   Washers (2)

*Note: Tighten the bolts so they are snug, but not too tight.  Do not draw the bracket and strap plates together.
[image: ]

6.056 Connect the cable for the actuator to the cable on the power supply.  Turn the power supply on.

[image: ] [image: ]

6.057 Remove the red clip from the actuator. Do not spin the actuator sleeve by hand.  Hold the actuator sleeve stationary (so it doesn’t rotate) and turn the knob on the power supply to the “Lower” position.  This will lower the end of the arm to the deck.  Fine adjust it when it gets close so that the hole in the actuator shaft lines up with the hole in the bracket.

[image: ]Holes line up


6.058 Place 2 plastic washers (E83145) on each side of the actuator arm.  Install a clevis pin (E28699) to connect the actuator arm to the deck.  Secure it with a cotter pin (E28671).  You may need to squeegee the bracket together to get the pin installed.

[image: ]

6.059 Manually cycle the deck up and down to make sure everything moves properly.  
6.060 If the machine is equipped with a Solichem system, get an assembled solution canister and a puck cage.  Place the puck cage into the canister.  Refer to the appropriate SOP for assembly instructions.  
6.061 Attach the tube to the machine using 2 loop clamps (E28969), 2 screws (E28648), and 2 washers (E28617).  Line it up so that the top cap is just above the upper clamp.  This will ensure that the lid does not interfere when it is closed.  Tighten the screws with care so not to strip the inserts.

[image: ]

6.062 Hold the supply hose from the pump up to the t-fitting on the solution canister assembly.  Try to match the slope with the hose in the photo.  You may need to trim about 1” off of the end.  Before connecting to the fitting, place a pinch clamp (E28773) onto the hose.  Once it is positioned properly, pinch it to secure.

[image: ] 

6.063 Cut a 12” piece of 3/8” hose (E28620).  Press one end of the hose onto the Y-Fitting on the scrub deck.  The other end goes to the outlet port of the solution canister.  Make the slope match the photo below.  You may need to trim some.  The y-fitting should still sit vertically.

[image: ]
6.064 Get a TDS Board assembly and 2 conductivity probes.  Refer to the proper SOP for how to build these.

[image: ] [image: ]

6.065 Install one of the probes into the feed line going from the canister to the deck.  Cut the hose about 5”-6” from the canister and install.  This will ensure the probe is close to the horizontal portion of the hose yet away from the motor when the deck is raised.  Point the body of the probe towards the back of the machine as shown.

[image: ]

6.066 Install the probe into the supply line from the pump.  The probe needs to be pointing upwards as best as possible.  Cut into the supply line close to the deck where the hose flattens out.  This will be about 8”-9” from the canister.  Install the ends of the T into each hose with a pinch clamp (E28773) over each.  Orient the probe as shown in the photo to make sure it will not hit anything as the deck goes up and down.  Pinch the clamps once it is oriented properly.
 [image: ]
6.067 Pop the rubber grommet out of the TDS box and pass the 4 pin terminal from the main wire harness through it and into the box.  Connect it to the proper terminal on the board.  Ensure that the jumper on the board has been removed.

[image: ]  [image: ]
6.068 Take the wire from the probe on the feed line to the deck and pass it over top of the pump supply line as shown.

[image: ]

6.069 Feed the ends of the probe wires through the hole in the bottom of the TDS Board box.  Connect the probes to the proper terminals.  Ensure that the probe terminal with the black line is connected to the board terminal with the black line.  Put the grommet back into the hole.
[image: ] [image: ]

6.070 Cut about 12” of 3/8” loom (E11213) and wrap it around the bare wires at the ends of the harness going into the shield bracket.  Feed the end of the loom through the grommet.
[image: ]

6.071 Mount the TDS Board to the inside of the head lift on the right side using 2 bolts (E29410) and 2 nuts (E28853).
[image: ][image: ]


6.072 [image: ]Connect the Low and Medium Pressure Switches to the appropriate terminals on the main wiring harness. (Assembler left side)Medium Pressure – Purple wire from Harness
Low Pressure – Blue wire from Harness


6.073 [image: ]Connect the High-Pressure Switches to the appropriate terminals on the main harness. (Assembler right side)Gray Wire from Harness


6.074 Be sure the harness passes in front of the actuator as shown.

[image: ]

6.075 [image: ]Disconnect the actuator from the power supply and connect it to the proper connector on the main harness.  Wrap the actuator wire around the harness to keep it from moving around.

6.076 Plug in the SB175 Anderson connector in the battery compartment.  Turn on the battery by pressing and holding the power button for 3-5 seconds.  Turn the key on and the deck should raise up.  Ensure all of the cables and hoses are still resting properly.

[image: ]   [image: ]

6.077 Wrap a skirt around the deck (E29341 for 26” / E29342 for 28” / E29343 for 32”).  Adjust the tension so that it is loose enough to float up and down but tight enough so that it doesn’t fall off.

[image: ] [image: ]







6.078 Refer to the appropriate SOP for instructions on how to assemble a Recovery Tank.
6.079 Place the tank near the machine using the cart shown.  This will angle it to allow it to be attached easier.  Bring the tank over to the machine and adjust the build cart height to allow the first hinge to be attached.

[image: ] [image: ]

6.080  Attach the first hinge using 2 flange bolts (E29569).  Once that is done, adjust the build cart height to allow the 2nd hinge to be attached.  Use 2 more flange bolts (E29569) to attach.  
[image: ] [image: ]



6.081 Close the recovery tank lid and verify that it is centered on the machine.  If not, open it back up and readjust by loosening the screws and move it.  Continue until it is centered.  **There is nothing keeping the recovery tank from falling all the way open.  Ensure either the cart is in place or there is another person helping hold it open if adjustment is needed.**
6.082 Attach the solution and recovery tanks using a recovery tank cable (E28760).  Attach each end of the cable using a hex bolt (E29392) and a hex nut (E12524).  Thread the bolt in part way, then tighten the nut to the tank to ensure the cable end can pivot.  **Note-Ensure that the cable loops down into the solution tank cavity as the lid is closed.  If it loops upward it could loop around the HEPA filter and tear if off.  If it loops up, either put a kink in the cable or turn one of the ends of the cable 180°.
[image: ] [image: ]
[image: ]
6.083 Install a HEPA filter (E29527) onto the vac motor using a worm clamp (E28755).  Use the provided torque screwdriver to tighten the clamp to 15 in-lbs of torque.  

[image: ] [image: ]

6.084 Connect the vac motor and the ground wires to the main wire harness.  Clean up the wiring in the tank using 2 zip ties (E83523).

[image: ]
6.085 Clean up the wiring in the battery compartment.  This step uses 2-3 zip ties (E83523).

[image: ] 

6.086 Take a squeegee vac hose (E29576) and press the angled end onto the barbed fitting on the back of the recovery tank.  
[image: ]  
6.087 Take a recovery tank drain hose (E28921) and attach it into the drain port of the recovery tank by using a worm clamp (E83966).
[image: ] 
6.088 Route the 2 hoses out of the battery compartment.

[image: ]



6.089 Connect the end of the squeegee vac hose to the port on the squeegee.  Hang the end of the recovery tank drain hose as shown.

[image: ] [image: ]

6.090 [bookmark: _Hlk198112719]Take a recovery tank lid (E28577).  Put a little blue silicone gasket maker into the groove in a couple points to hold the gasket in place.  Be sure to put some under each end of the gasket.  Cut a 7’ length of gasket (E29528) and install it into the groove.  The edge with the rounded bulb goes towards the outside of the lid.  Trim as needed to get the ends to line up.
[image: ] [image: ]Ends meet here

6.091 Attach the lid to the tank using 2 shoulder bolts (E29558).  

[image: ]

6.092 Attach a debris tray (E29525) to a puck holder (E29561) and place them into the pocket in the tank.

	[image: ] [image: ]	



6.093 Close the recovery tank lid.
6.094 Do a quick functional check of the unit to make sure all of the functions work prior to sending the machine to QC.
6.094.1 Verify vac motor turns on and off as required.  
6.094.2 Verify head lift goes up and down.  The head lift switches are not yet set but moving the knob to down pressure 1 should start it moving down.  Once you verify it moves down, turn the knob back to the UP position and it will retract.
6.094.3 Ensure the wheels are chocked and quickly check the transaxle.  Turn the speed knob all the way down and pull the bail.  You should feel the machine try to move.

7 References (optional section as needed)
7.01 
8 Training Guide

	Functional Training Groups Requiring Training

	Equipment Assembly Group

	



9 SOP Change Control

	Date of Change
	Reason for Change

	Rev 01 – 1/20/2026
	This is the first version of the S.O.P. hence there are no revisions to this document.
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