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1 Purpose
1.01 The purpose of this document is to describe the procedure to properly operate the Indeva Lift Assists in the Plant 2 assembly area.

2 Scope 
2.01 This Standard Operating Procedure (SOP) applies to Manufacturing Team Members at Betco Corporation Ltd.

3 Responsibilities
3.01 The operations manager/supervisor is responsible for enforcing this SOP.

4 Materials 
4.01 NA

5 Procedure

Procedure to use the tool head in “Handle Mode” (Standard)
5.01 When the lift assist tool head is at rest with the E-stop activated, the display will show the word “Stop”.  At this point, the tool head is locked and will not move up or down.
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5.02 To use the lift assist, release the E-stop on the opposite side of the tool head by twisting it clockwise.  The display will read “Abil”.
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5.03 Keeping your hand off of the handle, press the “RESTART” button on the tool head.  The display will now read “on”.  

[image: ] [image: ]

5.04 The tool head is now active.  Grab the handle and move the tool head to the desired location.  NOTE: The first move made after grabbing the handle needs to be upwards.  This is a safety precaution.  The tool head will only move when your hand is on the handle.
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5.05 Hook onto the objects lifting points using the clips provided on the tool head.  Grab the handle again and move the object to the desired location, set the object down and release the clips.
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5.06 When not using the tool head, store it in a position that will be out of the way.
5.07 Push in the E-stop to lock the tool head.

Using the tool head in “Float Mode”

5.08 When the lift assist tool head is at rest with the E-stop activated, the display will show the word “Stop”.  At this point, the tool head is locked and will not move up or down.
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5.09 To use the lift assist, release the E-stop on the opposite side of the tool head by twisting it clockwise.  The display will read “Abil”.
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5.010 Keeping your hand off of the handle, press the “RESTART” button on the tool head.  The display will now read “on”.  
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5.011 The tool head is now active.  Grab the handle and move the tool head to the desired location.  NOTE: The first move made after grabbing the handle needs to be upwards.  This is a safety precaution.  The tool head will only move when your hand is on the handle.
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5.012 Hook onto the objects lifting points using the clips provided.  Lift the object upwards so its weight is supported by the lift and release the handle.  
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5.013 If float mode is desired, press the “RESTART” button again while keeping your hand off of the handle.  A green light will light up (SHOWN BELOW).  
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5.014 Float mode does not require your hand to be on the handle to move the tool head.  When in float mode, you can grab the object you are lifting and move it that way.  The lift assist will sense your movement and react accordingly.
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5.015 Move the object to the desired location, set it down, and release the clips.  NOTE: Grabbing the handle at any point while in Float Mode will de-activate Float Mode.  The unit will immediately go back into Handle Mode (Steps 4.01-4.09).
5.016 When not using the tool head, store it in a position that will be out of the way.
5.017 Push in the E-stop to lock the tool head.













6 Training Guide

	Functional Training Groups Requiring Training

	

	

	



7 SOP Change Control

	Date of Change
	Reason for Change

	Rev 01 -  2/14/2014
	This is the first version of the S.O.P. hence there are no revisions to this document.

	Rev 02 - 1/22/2018
	Added Responsibilities Section
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