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1 Purpose
1.01 The purpose of this document is to describe the procedure for assembling an Optima Propane Burnisher front pulley.
2 Scope 
2.01 This SOP applies to all equipment assembly team members.  The process applies to the following machines:
E012800EQM0600BE1200 – 21” Optima XR
E012805EQM0600BE1200 – 21” Optima XR w/ Clutch
E012815EQM0600BE1200 – 21” Optima XR w/ Emissions & Clutch
E012830EQM0600BE1200 – 27” Optima XR
E012835EQM0600BE1200 – 27” Optima XR w/ Clutch
E012840EQM0600BE1200 – 27” Optima XR w/ Emissions
E012850EQM0600BE1200 – 27” Optima XR w/ Dust Control
E012860EQM0600BE1200 – 27” Optima XR w/ Clutch & Dust Control
E012865EQM0600BE1200 – 27” Optima XR w/ Emissions & Dust Control
E012875EQM0600BE1200 – 27” Optima XR w/ Emissions, Clutch, & Dust Control
3 Responsibilities
3.01 The operations manager/supervisor is responsible for enforcing this SOP.
4 Materials 
4.01 The proper materials needed for this process are listed on the machine work order.
5 Definitions
5.01 
6 Procedure 
6.01 The pulley that is used is different depending on what size machine is being assembled.  Use 12401 for a 27” machine or 12981 for a 21” machine.  Once the correct pulley is selected, hand assemble it and a bushing (12400).  The screw and washer needed should be provided with the bushing. Install the screw and washer finger tight at this point.  
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7 References (optional section as needed)
7.01 
8 Training Guide

	Functional Training Groups Requiring Training

	Equipment Assembly Group

	



9 SOP Change Control

	Date of Change
	Reason for Change

	Rev 01 - 11/22/2013
	This is the first version of the S.O.P. hence there are no revisions to this document.

	Rev 02 - 1/12/2018
	Added Responsibilities Section

	Rev 03 - 5/4/2018
	Updated for the Optima XR upgrade

	Rev 04 - 3/21/2025
	Removed work center notes
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Management Approval:______________________________________ Date:______________________
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