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1 Purpose
1.01 The purpose of this document is to describe the procedure for assembling an Optima Propane Burnisher motor pulley.
2 Scope 
2.01 This SOP applies to all equipment assembly team members.  The process applies to the following machines:
E012800EQM0600BE1200 – 21” Optima XR
E012830EQM0600BE1200 – 27” Optima XR
E012840EQM0600BE1200 – 27” Optima XR w/ Emissions
E012850EQM0600BE1200 – 27” Optima XR w/ Dust Control
E012865EQM0600BE1200 – 27” Optima XR w/ Emissions & Dust Control
3 Responsibilities
3.01 The operations manager/supervisor is responsible for enforcing the SOP.
4 Materials 
4.01 The proper materials needed for this process are listed on the machine work order.
4.02 Hand/Power Tools
5 Definitions

6 Procedure 
6.01 Assemble the drive pulley assembly.  This consists of a pulley (12546) and a bushing (12547).  Three bolts and lock washers should be supplied with the bushing.  Insert the bushing into the pulley and line the holes up.  The pulley and bushing are tapered so they will only assembley one way.  Attach the two pieces with the bolts and washers.  Finger tight is all that is needed at this point. 
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7 References (optional section as needed)
7.01 
8 Training Guide

	Functional Training Groups Requiring Training

	Equipment Assembly Group

	



9 SOP Change Control

	Date of Change
	Reason for Change

	Rev 01 - 11/22/2013
	This is the first version of the S.O.P. hence there are no revisions to this document.

	Rev 02 - 1/12/2018
	Added Responsibilities Section

	Rev 03 - 5/4/2018
	Updated for the Optima XR upgrades

	Rev 04 - 3/21/2025
	Removed work center notes and updated machine ID’s in Scope 2.01
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5 Procedure
5.01 Assemble the drive pulley assembly. This consists of a pulley (12546) and a bushing (12547),
Three bolts andlock washers shouldbe supplied withthe bushing, Insert the bushing into the
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