 (
Technical Bulletin 20090326-1
) (
Battery Level Indicator FUNCTION
The battery 
level indicator is 
a device that helps protect the machine’s batteries from damage cause by over discharging the batteries.  The indicator also lets the machine operator know when the batteries need to be recharged.  When the machine is turned on, the battery level indicator continuously monitors the battery voltage.  Typical output of the indicator is as follows:
If the battery 
voltage is below the 
shutdown 
voltage, the machine will 
either be turned off or will not be able to start
.
  If the machine is in operation when the shutdown voltage is reached, the outside (right most) yellow LED will flash for 15 seconds and then the red LED, “D”, will be turned on.  The machine will be turned off automatically.  The batteries should be charged.
If the 
battery 
voltage is 
at a satisfactory state of charge, some number of the yellow LEDs will turn on.  The increasing qualities of illuminated yellow LEDs indicate higher states of battery charge.  The 
machine will 
be able to be turned on and operated
.
If the 
battery 
voltage 
is above, but is very close to the shutdown voltage when the machine is turned on, some of the yellow
 
LEDs
 will 
flash and the batteries will be charged before the machine is placed into operation.
SETTING the Battery Level
 Indicator 
Shutdown Voltage
Turn the machine off and disconnect the batteries.  Locate the rotary selector switch located on the back of the Battery Level Indicator.  
The rotary selector switch
 is switch “A” shown in the diagram above.  Gently rotate the switch so that the arrow is pointing at the number 3.  Doing this sets the system shutdown voltage to 31.68 VDC.  Never set the selector switch to any other position because battery damage or decrease opera
ting time will be experienced.
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