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	Technical Bulletin
Crewman AS20B Charger Connection Instructions



1 Remove the top cover the recovery tank to get access to the red plug.
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2 Pull on the red handle to disconnect the battery pack from the machine.
3 The end of the plug that is mounted to the tank leads to the control panel.  Do not hook the charger to this plug.
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4 The end with the handle leads to the battery pack.  You will see a green line on each side of the plug.
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5 Ensure that the charger being used has a green “QC Approved” sticker on it.
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6 The red plug on the charger has the same 2 green lines as the connector that goes to the battery pack.
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7 Plug the charger into the battery connector.  Ensure the two connectors with the green lines are what you connect.  Remember: Green to Green.
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8 The charging cycle will now begin.
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