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Sales and Service Managers:





This bulletin is to notify you of a “Battery Type” selection option on part #83323-00 Battery Charger for the BPS26 Battery Powered Sweeper.  



















































































Should you have any questions please contact our Technical Support Team:


        �                      �





























To: 		Authorized Betco Equipment Distributors


From: 	Chris Keene – Category Manager


Subject: 	Betco BPS26 Battery Powered Sweeper Charger Settings 





The BPS26 Battery Powered Sweeper utilizes wet lead acid batteries therefore it is important that the proper charger setting is selected. As shown in figure 1, the selector is located on the front of the charger near the center. See figure 2 for a closer view.





Note – Using the wrong setting will cause the batteries to not charge properly and negatively affect overall run times of the machine.
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Figure 2. 
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Note- The switch should be set to the up position for wet lead acid batteries.
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Figure 1.
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