1. Remove the front housing cover from the machine.
2. Remove the pad driver. Use a ¾” combination wrench placed on top of the bearing housing shaft to secure it in place (ref#1). Spin the pad driver assembly counterclockwise (ref#2). This will loosen the driver for easy removal (ref#3). 
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3. Using a 5/8” combination wrench or socket, remove the two right side bearing housing bolts completely (ref#4). Note- The right hand side is defined as when standing in the operators’ position.
4. Loosen the two left side bolts enough to allow the bearing housing to release its grip on the spacers (ref#5 & #6).

[image: image4.jpg]


  [image: image5.jpg]


  [image: image6.jpg]



5. With the machine tilted back, the spacers should fall out from between the deck and bearing housing. A magnetic tool can be used in the event they do not come out on their own (ref#7). Visually check to make sure all spacers are removed from between the deck and housing.
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6. Replace the right-rear bolt – do not tighten.
7. Position (1) ½” SAE (2mm thick) spacer between the deck and the bearing housing at the front right bolt position, put the bolt back in place.

8. Tighten all bolts beginning with the right side bolts first, then the left side bolts.
9. Install the pad driver assembly by spinning back on in a clockwise motion.
Betco/PowerBuff Service Technician Contact List:

Bill Brand

Phone # 888-462-3826 Ext. 3048

Mobile # 419-290-3251

Pete Samuelson

Phone # 888-462-3826 Ext. 3503

Mobile # 419-290-5417

Ed Stoner

Phone # 336-627-0111 Ext.105
Mobile # 336-707-3498

#7











#4





#5





#2





#1





#3











#6








