
                                 Check ohms between these two pins set .2  to .5 ohms
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Loosen set screw with 2MM allen wrench  (remove Cover cap first)
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With set screw loose, ohm meter connected to pins shown above, rotate shaft to set ohms, clockwise less - counterclockwise more.
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