Propane Testing

Honda co% = .01-.05 turn the Set screw in bottom regulator counterclockwise to lower co%.

Kawasaki co%= .01-.04. If the Kawasaki Doesn’t Start turn the set Screw clockwise. 

Rpm should be no Higher than 3700. No lower than 1800
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