Propane Burnisher – Regulator Set-Up Process
Tools Needed: Engine tachometer, CO emission analyzer, Phillips head screwdriver, 3/32” Allen wrench.

1. Position regulator set screw to just below the inside ridge of the regulator housing.
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2. Set throttle control to lowest speed and adjust engine RPM to 1480-1520.  RPM should first be adjusted at the carburetor, then at the throttle linkage.
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3. Begin screwing in the regulator idle control screw, ½ turn at a time, until the engine RPM reaches 1560-1600.
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4. Check CO emissions at this idle speed.  CO emissions should be <100PPM.

5. Move the throttle control to full speed.  Engine RPM should be >3500.
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6. Check Co emission at full speed.  CO emissions should be <100PPM.

7. Install the regulator idle screw plug provided with the regulator. 
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