Vacuum Delay on Stealth 20B/BT before serial number beginning 21500000

To disable vacuum on until key off feature when squeegee is raised, locate jumper on relay board labeled ECB
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Remove Jumper
[image: ]
Vacuum Motor will now turn off as soon as the squeegee is lifted off of the floor
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