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CAUTION

Battery acid is dangerous. Wear eye and face protection, hand protection,
and body protection when working on and around batteries. If you get
acid on your skin, wash off immediately. If you get acid on your clothing,
remove clothing and wash any skin that was in contact with the clothing.
Baking soda mixed with water will help to neutralize the acid on your skin.

The machine is very heavy, so be very careful when loading, transporting,
and unloading the machine

Keep all body parts, clothing, and objects away from moving parts.
Operate machine from the rear, not from the side.

Disconnect a wire to the batteries before working on the machine.
Do not operate machine with charger plugged in.

Do not operate machine with any parts damaged or missing.

Do not operate close to stairs, loading docks, or other drop-offs. Do hot
park machine in such a manner that it could roll, forward or backward, off
a drop-off.

Authorized personnel must perform maintenance and repairs. Do not alter
or modify the machine, unless authorized by the manufacturer.

Do not expose the electrical components to water or excessive moisture.

Always put caution signs around the areas that are being cleaned.

Do not use machine as a “ladder”. Do not use machine as a “forklift" to
push stuff around. Do not ride or let anyone ride on the machine.

Your machine warranty may be voided if parts other than PowerBuff parts
are used.




WARNING:  TO CHARGE; PLUG CONNECTOR INTO BURNISHER, THEN PLUG CHARGER INTO WALL OUTLET.   WHEN FINISHED, REMOVE WALL OUTLET PLUG FIRST, THEN BURNISHER CONNECTOR.








