Pete,

Yes, as follows:

E01 - When maximum battery voltage is reached.

E02 – Over temperature

E03 – Exceeded time of charging phase – This could happen with a shorted cell in the battery set.

SCt – Safety timer operation

Srt – Internal short circuit

When first plugged in, the charger will show consecutively on it’s display -  SPE – voltage – Amps – Charging Curve # -- GEL or Acd

If the charger is not connected to the battery it will show Bat

Please let me know if you need more information.

