Fault Finding

The MillipaK controller includes a number of features designed to help the user track down

operational faults, wiring faults or internal controller faults.

The Diagnostic LED mounted next to the calibrator connectors on the front of the controller

serves as a simple diagnostic tool as explained below:

ON No fault, normal condition Handle Switch
OFF Internal controller fault

1  flash Personality out of range

2  flashes Illegal start condition

3  flashes MOSFET Short Circuit Internal
4  flashes Contactor fault Loose Wire or bad relay
5  flashes Not used

6  flashes Accelerator wire off fault

7  flashes Low or High battery voltage

8  flashes Over temperature or timed cutback

9  flashes Rotor Position Sensor Fault Loose wire, bad solinoid
