This is the bottom of a PB 28 propane with the pad driver off. (this is the way we ‘used’ to make them.  On the left is the 10” pulley [E010428], the ‘tensioner’ has the orange part in the center.  It IS shown on the Deck drawing as item 13 [E010459].  Note: the deck drawing also has a reference for the ‘tensioner pulley’ (black and orange part) [E012353].

The more solid pulley, on the end of the motor shaft and positioned between the wheels is the old BC 35 pulley [E012295]. This arrangement used the BX 50 Belt [E012446].
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We have stopped using the BC 35 as of unit number 11860 and now use the sheave/bushing arrangement shown below. This requires a BX 51 belt [E010472]

[image: image2.jpg]



Hope this is clearer.  Ed

