2mm Washer installation on XT21 wheel brackets


Instructions for “in field” adjustments to XT21 burnisher:

1. Lift and support rear of machine in a safe manner, until wheel is off the ground. Figure 1.
2. Using either; two - ½ inch wrenches or; one ½ inch wrench and a socket (better because you can use it on the bracket nuts), remove the bolt and nut that serve as an axle, and remove the wheel.  Figure 2.

3. Using a wrench on the topside of the deck, (Figures 4-left & 4-right) and the socket/ratchet on the underside of the deck, take the nuts off between the bracket legs.  Figure 3.
4. Position one washer over each drilled hole on the bracket. Figure b. (you may want to use a small amount of adhesive, or tape,  to keep the 4 washers in place while replacing the bracket).
5. Place the bracket up against the deck so all four bolts are sticking through the holes and install the flat washer and lock-nut on each bolt. 
6. Install the wheel with its bolt and nut IN THE MOST FORWARD POSITION. 
Figure 5a/
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   Figure 1. Lift and support machine until wheel is off ground.
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   Fig. 2. Remove wheel - requires ½ in. wrench(s) &/or socket.
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 Figure 3.                         [image: image4.jpg]


 Figure 4-left.                       Left side Bracket removal… (note: this picture already has washers between bracket and deck – using for example.  Yours should look like this when reassembling)..
[image: image5.jpg]
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Figure 5a                         Figure 5b

On Right side, you will need to use open end of wrench to hold the bolt head where the motor interference is encountered.

Tools & Equipment needed:

a. 2 – short 2” x 4”s

b. 2 – ½ inch combination wrenches, or 1 ½ inch combination wrench and a ½ inch socket/ratchet w/extension.

c. 4 – 2mm flat washers (SAE ½ inch flat washers - ~.085” thick)
Bonus information – serial number location [image: image8.jpg]


 very hard to see.
1 Washer between deck and bracket on each bolt





Note: Wheels in forward position.











