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1 Purpose
1.01 The purpose of this document is to describe the procedure for assembling the Orbital Head on the Genesys Machine.
2 Scope 
2.01 This SOP applies to all equipment assembly team members.  The process applies to the following machine ID’s:
EP50289EQS0600BE1200 – Orbital Head Assembly
3 Responsibilities
3.01 The operations manager/supervisor is responsible for enforcing this SOP.
4 Materials 
4.01 The proper materials needed for this process are listed on the machine work order.
5 Definitions
5.01 
6 Procedure
6.01 Place the base (E28896) on a motor (E28521) in the orientation shown and attach it using 4 bolts (E83914) and 4 flat washers (E28617).  Use Blue Loctite on the threads.  Tighten the bolts to 7ft-lbs min.  Mark the orientation of the bolt heads once complete.  
Motor wires point this direction.














6.02 Place a machine key (E28635) into the motor shaft.

6.03 [image: ]Place some anti-seize on the motor shaft.  Place a bearing/counterweight assembly (refer the proper SOP for assembly instructions) onto the motor shaft and attach it using a hub washer (E28631) and a hex bolt (E29426).  Use Blue Loctite on the threads. Using the blue torque gun with ½” socket tighten the bolt to 15 ft-lbs min. A green light will appear when torque is good, if red light appears removed bolt repeat process. Mark the orientation of the bolt head. 	

6.04 Take a water feed manifold (E28898) and press a hole plug (E28535) into each end of it.
[image: ]
6.05 Before attaching the manifold, run a die over the 2 studs on the deck.  The treads can be damaged or have paint on them.  Attach the manifold to the base with 2 loop clamps (E28534) and 2 nylock nuts (E28853).  The center feed port should line up with the large hole in the base.  To help with alignment, you may want to use a barbed elbow and put it through the deck and into the tube.  Ensure that the holes in the manifold are oriented properly.  When the center hole is aligned, they should slightly point towards the front of the deck.  
[image: ] [image: ]Barbed Elbow
Holes should be angled slightly towards the front

6.06 Attach 2 bumper casters (E28509) to the weldment in the appropriate locations.  Put a bushing (supplied with the wheel) into the ID of the wheel.  Sandwich a spring washer (E28640) between the wheel and the plate.  Use a flat head screw (E28634), a washer (E28622), and a nylock nut (E28623) to attach the wheel.  Ensure the wheel still spins once installed.
[image: ]
6.07 Take 4 isolators (E28530) (drill out holes of isolators before installation to clean them out) and place a spacer (E28633) over the threaded stud on each one.  Attach the isolators to the deck by putting the studs through the appropriate holes and attaching them using a nylock nut (E81063) and a flat washer (E28622).
[image: ] [image: ]  [image: ]
6.08 Place an o-ring (E28527) into the groove on the orbital bearing hub.
[image: ]O-Ring goes in this groove


6.09 [image: ]Place an orbital pad driver plate (E28897) into position and attach it.  Use 4 flat head screws (E28763) to attach the plate to the bearing assembly.  Then, use 4 flat head screws (E28639) to attach the plate to the isolators.  Use Blue Loctite on all threads.

6.010 [image: ][image: ]Stick a pad driver face (E28889) to the plate followed by a red pad (E89831).
 
6.011 Flip the base over.
6.012 Push 2 wire tie mounts (E28621) into the appropriate holes on the weldment next to the watering port.




6.013 Cut a 24” piece of 3/8” hose (E28620).  Press the hose onto the end of a plastic elbow (E28536) and install the other end of the elbow into the top side of the manifold.  
6.014 [image: ]Secure the hose and elbow with 2 zip ties (E83523).

6.015 [image: A metal plate with holes and screws

Description automatically generated]Place an orbital head lift bracket (E28981) on the table.  Look at the threads on the studs and run a die over them to clean them up if needed.












6.016 Take a left-hand head bracket (E28860) and verify with the picture (in step 18) that the brackets are facing correctly.   Attach the bracket to the studs on the head lift bracket using 2 flat washers (E28622) and 2 nuts (E81063).  Leave the nuts loose at this point.
6.017 Repeat the process for the right-hand head bracket (E28859) 
6.018 [image: A metal plate with a round hole

Description automatically generated]Attach (E28861) bracket on the threaded studs (closest to the motor) using 2 hex nuts (E28618) leave loose at this point. Verify correct orientation of bracket in should be angling down to front of lift bracket. Next place a bushing (E28531) into the top and bottom of each of the 4 mounting holes. Then place isolator bushing (E28656) through each pair.






6.019 [image: A machine with a tube and screws

Description automatically generated]Lay the head lift bracket assembly onto a motor bracket weldment then fish the wires and the hose through the openings in the plate. Next attach it using 4 hex bolts (E29553), 4 large washers (E28764), and 4 flat washers (E28622).  Use Blue Loctite on the bolt threads.  Tighten until the isolators start to mushroom.  


7 References (optional section as needed)
7.01 
8 Training Guide

	Functional Training Groups Requiring Training

	Equipment Assembly Group

	







9 SOP Change Control

	Date of Change
	Reason for Change

	TBD
	This is the first version of the S.O.P. hence there are no revisions to this document.
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