CBHF2-PFC battery Charger

DIP Switch Settings

* Dip1 Dip2 Dip3 Dip4 for the selection of the CHARGING CURVE

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Dip1** | **Dip2** | **Dip3** | **Dip4** | **Charging Curve** |
| ON | ON | ON | ON | 0 |
| OFF  957756 | ON | ON | ON | 1  (curve for Lead-acid (Wet) traction  batteries) |
| ON | OFF | ON | ON | 2  IU0U-AGM for ZENITH Batteries |
| OFF | OFF | ON | ON | 3 |
| ON | ON | OFF | ON | 4 |
| OFF | ON | OFF | ON | 5  IUU0-AGM for FULLRIVER AGM batteries |
| ON | OFF | OFF | ON | 6  (curve for Sealed Lead-acid and GEL  batteries from Trojan and other  manufacturers) |
| OFF | OFF | OFF | ON | 7 |
| ON | ON | ON | OFF | 8 |
| OFF | ON | ON | OFF | 9 |
| ON | OFF | ON | OFF | 10  IUIa-OPTIMA for OPTIMA Batteries (12V only) |
| OFF | OFF | ON | OFF | 11  (curve for GEL batteries from Sonnenschein, DETA and other  manufacturers) |
| ON | ON | OFF | OFF | 12 |
| OFF | ON | OFF | OFF | 13  IUU0-OPTIMA for OPTIMA  Batteries (24V,36V and 48V only) |
| ON  957756-1 | OFF | OFF | OFF | 14  IUIa-AGM for DISCOVER Batteries |
| OFF | OFF | OFF | OFF | 15 |