CBHF2-PFC battery Charger

DIP Switch Settings

* Dip1 Dip2 Dip3 Dip4 for the selection of the CHARGING CURVE

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Dip1** | **Dip2** | **Dip3** | **Dip4** | **Charging Curve** |
| ON | ON | ON | ON | 0 |
| OFF957756 | ON | ON | ON | 1(curve for Lead-acid (Wet) traction batteries) |
| ON | OFF | ON | ON | 2IU0U-AGM for ZENITH Batteries |
| OFF | OFF | ON | ON | 3 |
| ON | ON | OFF | ON | 4 |
| OFF | ON | OFF | ON | 5IUU0-AGM for FULLRIVER AGM batteries |
| ON | OFF | OFF | ON | 6(curve for Sealed Lead-acid and GEL batteries from Trojan and other manufacturers) |
| OFF | OFF | OFF | ON | 7 |
| ON | ON | ON | OFF | 8 |
| OFF | ON | ON | OFF | 9 |
| ON | OFF | ON | OFF | 10IUIa-OPTIMA for OPTIMA Batteries (12V only) |
| OFF | OFF | ON | OFF | 11(curve for GEL batteries from Sonnenschein, DETA and other manufacturers) |
| ON | ON | OFF | OFF | 12 |
| OFF | ON | OFF | OFF | 13IUU0-OPTIMA for OPTIMA Batteries (24V,36V and 48V only) |
| ON957756-1 | OFF | OFF | OFF | 14IUIa-AGM for DISCOVER Batteries |
| OFF | OFF | OFF | OFF | 15 |