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Initial:

1. Start with a handle tower weldment (88596).
 SHAPE  \* MERGEFORMAT 



2. The handle adjust gear (88598) and the handle pivot shaft hub (88593) are then attached to the handle tower weldment using 6 screws (88751).
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