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1 Purpose
1.01 The purpose of this document is to describe the procedure for assembling the TDS Board for all Genesys machines with SoliChem.  
2 Scope 
2.01 This SOP applies to all equipment assembly team members.  The process applies to all the Genesys machines with the SoliChem option
3 Responsibilities
3.01 The operations manager/supervisor is responsible for enforcing this SOP.
4 Materials 
4.01 The proper materials needed for this process are listed on the machine work order.
5 Definitions
5.01 
6 Procedure
6.01  Take a TDS board (E28784).  Remove the jumper shown.
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6.02 Take a TDS Shield Bracket (E28778).  Place a spacer (E29373) over each of the 4 studs in the 
bracket.  Place the TDS Board over the studs and secure it with 4 nuts (E29381).  Note the orientation of the board to the hole in the box.  
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7 References (optional section as needed)
7.01 
8 Training Guide

	Functional Training Groups Requiring Training

	Equipment Assembly Group

	



9 SOP Change Control

	Date of Change
	Reason for Change

	TBD
	This is the first version of the S.O.P. hence there are no revisions to this document.

	8/13/2021
	Added QC Checks and added probe installation

	10/26/2021
	Remove probe installation

	11/6/2023
	Updated current process
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