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1 Purpose
1.01 The purpose of this document is to describe the procedure for assembling a propane burnisher pad driver.
2 Scope 
2.01 This SOP applies to all equipment assembly team members.  The process applies to the following sub-assembly’s:
EP50040EQS0600BE1200 – Flex lok assembly 27” complete
EP50027EQS0600BE1200 – Flex lok assembly 24” complete
EP50028EQS0600BE1200 – Flex lok assembly 21” complete
3 Responsibilities
3.01 The operations manager/supervisor is responsible for enforcing this SOP.
4 Materials 
4.01 The proper materials needed for this process are listed on the sub-assembly work order.
4.02 Hand/Power Tools
4.03 Riveter
5 Definitions
5.01 
6 Procedure 
6.01 Start by bolting the shaft plate (10586) to the flex-lok (10252 for 27”, 10251 for 24”, or 10250 for 21”) using 6 bolts (10112), lock washers (81067), flat washers (12444), and nuts (81063).
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6.02 Unscrew the top and bottom pieces of the center-lock.  Attach the appropriate half of the center lock (12517) to the flex-lok using 3 rivets (10850) and the pneumatic riveter.  Use the three holes shown in the picture below.
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6.03 Place a burnishing pad (84627 for 27”, 84624 for 24”, or 84621 for 21”) onto the gripping side of the flex-lok.  Center the pad as best as possible.
[image: ]Burnishing Pad

6.04 Thread the remaining half of the center lock into the center of the pad driver.  Thread it until the 2 halves start to ratchet together.  
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7 References (optional section as needed)
7.01 
8 Training Guide

	Functional Training Groups Requiring Training

	Equipment Assembly Group

	



9 SOP Change Control

	Date of Change
	Reason for Change

	Rev 01 - 11/18/2013
	This is the first version of the S.O.P. hence there are no revisions to this document.

	Rev 02 - 1/12/2018
	Added the Responsibilities section

	Rev 03 - 3/21/2025
	Removed work center note
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