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1 Purpose
1.01 The purpose of this document is to describe the procedure for assembling the wheels of an Optima Propane Burnisher.
2 Scope 
2.01 This SOP applies to all equipment assembly team members.  The process applies to the following machines:
E012800EQM0600BE1200 – 21” Optima XR
E012805EQM0600BE1200 – 21” Optima XR w/ Clutch
E012815EQM0600BE1200 – 21” Optima XR w/ Emissions & Clutch
E012830EQM0600BE1200 – 27” Optima XR
E012835EQM0600BE1200 – 27” Optima XR w/ Clutch
E012840EQM0600BE1200 – 27” Optima XR w/ Emissions
E012850EQM0600BE1200 – 27” Optima XR w/ Dust Control
E012860EQM0600BE1200 – 27” Optima XR w/ Clutch & Dust Control
E012865EQM0600BE1200 – 27” Optima XR w/ Emissions & Dust Control
E012875EQM0600BE1200 – 27” Optima XR w/ Emissions, Clutch, & Dust Control
3 Responsibilities
3.01 The operations manager/supervisor is responsible for enforcing this SOP.
4 Materials 
4.01 The proper materials needed for this process are listed on the machine work order.
4.02 Hand/Power Tools
5 Definitions
5.01 
6 Procedure 
6.01 The wheel brackets should be assembled in pairs as they are mirror images of each other.  Start with the wheel (12689).  Be sure to include a sleeve bearing that is supplied with the wheel but is probably stored separately.  This bearing goes inside the ID of the wheel.
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6.02 Take the wheel, a wheel bracket (86225), a bolt (10902), and a nut (10141) and bolt them all together.  On the wheel bracket are two holes.  Use the one that is closest to the edge for a 27” machine.  Use the other hole for a 21” machine.
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6.03 Bolt together the opposite wheel bracket.  All is the same except that the bolt should point the opposite direction.  The completed assemblies should be mirror images of each other.
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7 References (optional section as needed)
7.01 
8 Training Guide

	Functional Training Groups Requiring Training

	Equipment Assembly Group

	




9 SOP Change Control

	Date of Change
	Reason for Change

	Rev 01 - 11/22/2013
	This is the first version of the S.O.P. hence there are no revisions to this document.

	Rev 02 - 1/15/2018
	Added Responsibilities Section

	Rev 03 - 5/4/2018
	Updated for the Optima XR upgrades

	Rev 04 - 3/21/2025
	Removed work center notes

	Rev 05 – 11/17/2025
	Updated applicable machine ID’s in section Scope 2.01
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