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1 Purpose
1.01 The purpose of this document is to describe the procedure for load testing a propane machine battery.
2 Scope 
2.01 This SOP applies to all equipment assembly team members.  The process applies to the following machines:
E012800EQM0600BE1200 – 21” Optima XR
E012805EQM0600BE1200 – 21” Optima XR w/ Clutch
E012815EQM0600BE1200 – 21” Optima XR w/ Emissions & Clutch
E012830EQM0600BE1200 – 27” Optima XR
E012835EQM0600BE1200 – 27” Optima XR w/ Clutch
E012840EQM0600BE1200 – 27” Optima XR w/ Emissions
E012850EQM0600BE1200 – 27” Optima XR w/ Dust Control
E012860EQM0600BE1200 – 27” Optima XR w/ Clutch & Dust Control
E012865EQM0600BE1200 – 27” Optima XR w/ Emissions & Dust Control
E012875EQM0600BE1200 – 27” Optima XR w/ Emissions, Clutch, & Dust Control
E012327EQM0600BE1200 – Big Bertha XSM30 Propane Stripping Machine Pkg
E088398EQM0600BE1200 – Lil Bertha XSM24 Propane Stripping Machine Package
3 Responsibilities
3.01 The operations manager/supervisor is responsible for enforcing this SOP.
4 Materials 
4.01 The proper materials needed for this process are listed on the machine work order.
4.02 Battery Load Tester
5 Definitions

6 Procedure 
6.01 Take a battery (89827) and clamp the terminals using the appropriate clamps on the load tester. 
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6.02 Verify that the voltage reading is acceptable.  It should read 12V or higher.
6.03 Press and hold the red button for a couple seconds until the needle stops moving.
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6.04 Verify that the needle stays in the green area at the 200CCA line.

[image: ]Needle should stay above this line


6.05 If the battery falls below, it is no good.
7 References (optional section as needed)
7.01 
8 Training Guide

	Functional Training Groups Requiring Training

	Equipment Assembly Group

	



9 SOP Change Control

	Date of Change
	Reason for Change

	Rev 01 - 11/22/2013
	This is the first version of the S.O.P. hence there are no revisions to this document.

	Rev 02 - 1/12/2018
	Added responsibilities section

	Rev 03 - 5/4/2018
	Updated for the Optima XR upgrades

	Rev 04 - 3/21/2025
	Removed work center notes and updated machine ID list in Scope 2.01
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