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	REF
	PART NO.
	QTY
	DESCRIPTION
	SERIAL NO.

FROM
	NOTES:

	1
	09129
	2
	BEARING, 3/4 NYLINER SI
	
	

	2
	35220
	2
	GASKET, MICRO SWITCH COVER
	
	

	3
	38275
	1
	HANDLE, CONTROL
	
	

	4
	57047
	2
	NUT, 1/4-20 HEX NYLOCK
	
	

	5
	57113
	4
	NUT, 5/16-18 HEX NYLOCK
	
	

	6
	57247
	2
	NUT, PLATE SWITCH MOUNTING
	
	

	7
	62726
	2
	PLATE, MICROSWITCH MOUNT
	
	

	8
	66293
	2
	PIVOT, HANDLE
	
	

	9
	66301
	2
	PLUG, 1.00 HOLE
	
	

	10
	70129
	2
	SCR, 1/4-20 X 3.00 HHCS
	
	

	11
	70245
	4
	SCR, 4-40 X 3/4 PPHMS
	
	

	12
	70302
	4
	SCR, 5/16-18 X 1.00 HHCS GR5
	
	

	13
	70351
	6
	SCR, 10-32 X 3/8 HHTR W/STAR
	
	

	14
	72093
	2
	SWITCH, MICRO
	
	

	15
	73913
	2
	SPACER, 7/8 OD X .78 ID X 1.375 L
	
	

	16
	73938
	2
	SPRING, EXT. .5D X 2.75L X .075W
	
	

	17
	87029
	4
	WASHER, 5/16 X 3/4 SS
	
	

	18
	87068
	12
	WASHER, 1/8 RIVET BACKUP
	
	

	19
	87090
	4
	WASHER, 1/4 X 3/4 FLAT
	
	

	20
	89186
	1
	WELDMENT, TOWER
	
	

	21
	140247
	1
	BAR, GRAB HANDLE LEFT
	
	

	22
	140248
	1
	BAR, GRAB HANDLE RIGHT
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	REF
	PART NO.
	QTY
	DESCRIPTION
	SERIAL NO.

FROM
	NOTES:

	1
	27757
	1
	CONSOLE, REAR
	
	

	2
	57189
	4
	NUT, 1/4-20 FLANGE LOCK
	
	

	3
	70251
	4
	SET SCR, 1/4-20 X 1.0 PLTD DL
	
	

	4
	70305
	4
	SCR, 5/16-18 X 3/4HHCSGR5PLTDL
	
	

	5
	70604
	6
	SCR, 10-32 X 5/8 PPHMS BLACK
	
	

	6
	70532
	6
	SCR, 10-32 X 1/2 PPHMS BLK
	
	

	7
	87029
	4
	WASHER, 5/16 FLAT SS
	
	

	8
	140133
	2
	BRACKET, RECOVERY HOSE
	
	

	9
	87018
	6
	WASHER, #10 X 9/16 OD
	
	

	10
	57030
	6
	NUT, 10-32 HEX NYLOCK
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	REF
	PART NO.
	QTY
	DESCRIPTION
	SERIAL NO.

FROM
	NOTES:

	1
	500160
	1
	LABEL, BETCO (LEFT)
	
	

	2
	500161
	1
	LABEL, BETCO (RIGHT)
	
	

	3
	500023
	1
	LABEL, SCRUBBER PANEL
	
	

	4
	500024
	1
	LABEL, CIRCUIT BREAKERS
	
	

	5
	500057
	1
	LABEL, BETCO LOGO 
	
	


NOTE:  SEE “SAFETY LABEL LOCATION” PAGE FOR SAFETY LABEL INFORMATION.
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	REF
	PART NO.
	QTY
	DESCRIPTION
	SERIAL NO.

FROM
	NOTES:

	1
	14606
	2
	BREAKER, 30A 250VAC 50VDC
	
	

	2
	14607
	2
	BREAKER, 25A 250VAC 50VDC
	
	

	3
	14717
	1
	BREAKER, 3A 250VAC 50VDC
	
	

	4
	14942
	1
	BOOT, 3/8 CIRCUIT BREAKER
	
	

	5
	27695
	1
	CONTROLLER, 24VDC PROPEL MTR
	
	

	6
	27858
	1
	CIRCUIT BOARD, SOLUTION/FLOAT
	
	

	7
	35210
	1
	GASKET, ELECTRIC PANEL
	
	

	8
	48072
	2
	KNOB, 1.06 OD X .25 ID W/SET SCR
	
	

	9
	54145
	1
	METER,24V BATTERY CHARGE LEVEL
	
	

	10
	54156
	1
	METER, 0-50 AMP DC
	
	

	11
	57047
	4
	NUT, 1/4-20 HEX NYLOCK
	
	

	12
	57104
	6
	NUT, 10-32 W/STAR WASHER PLTD
	
	

	13
	57105
	3
	NUT, 1/4-20 HEX W/STAR
	
	

	14
	57106
	2
	NUT, 8-32 HEX W/STAR
	
	

	15
	57117
	6
	NUT, 5/16-24 HEX PLTD
	
	

	16
	57256
	2
	NUT, 6-32 HEX BRASS
	
	

	17
	62283
	1
	PLATE, METER RETAINING
	
	

	18
	62808
	1
	PLATE, ELECTRIC PANEL
	
	

	19
	66321
	1
	PLUG, .875 HOLE
	
	

	20
	67393
	3
	RELAY, 24VDC 100 AMP
	
	

	21
	70011
	1
	SCR, 1/4-20 X 5/8 HHCS  SS  DL
	
	

	22
	70067
	8
	SCR, 6-32 X 3/8 PPHMS SS
	
	

	23
	70393
	1
	SET SCR, 1/4-20X 1.25L
	
	

	24
	70615
	2
	SCR, 6-32 X 3/8 SRHMS BR
	
	

	25
	72130
	2
	SWITCH, SPST 2-POSITION ROCKER
	
	

	26
	72159
	1
	SWITCH, KEY 2 POSITION
	
	

	27
	72165
	1
	SWITCH, DPDT 3-POSITION ROCKER
	
	

	28
	73987
	1
	SHUNT, DC AMM. 25 AMP, 50 MV
	
	

	29
	73538
	2
	STANDOFF, 5/8 L, 6-32
	
	

	30
	73659
	1
	STANDOFF, INS. 1.0L, 1/4-20 THD
	
	

	31
	73734
	2
	SPACER, .166 ID X .313 OD X .375L AL
	
	

	32
	80845
	4
	BOOT, 3/8 CIRCUIT BREAKER
	
	

	33
	87026
	2
	WASHER, #6 LOCK EXT STAR  SS
	
	

	34
	87134
	8
	WASHER, #6 SPLIT
	
	

	35
	87142
	6
	WASHER, .344X.69X.066 FLAT PLT
	
	

	36
	87166
	6
	WASHER, 5/16 EXT LOCK PLTD
	
	

	37
	87187
	2
	WASHER, #6 FLAT BRASS
	
	

	38
	66335
	REF
	POTENTIOMETER
	
	SERVICE ONLY
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	REF
	PART NO.
	QTY
	DESCRIPTION
	SERIAL NO.

FROM
	NOTES:

	1
	E87557
	1
	COVER, FRONT DK GRY
	
	

	2
	E87664
	2
	KNOB, 5/16-18 4 PRONG
	
	

	3
	70639
	4
	SCR, 5/16 X 1.75 SSSCU
	
	

	4
	E87623
	2
	WASHER, 5/16 FLAT SS
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