SQUEEGEE GROUP – 28 IN SCRUBHEAD
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REF
PART NO.
QTY
DESCRIPTION
SERIAL NO.

FROM
NOTES:

1
57047
4
NUT, 1/4-20 HEX NYLOCK



2
57111
2
NUT, 3/8-16 HEX



3
57119
6
NUT, 3/8-16 HEX NYLOCK



4
57269
2
NUT, 3/8-16 HEX COUPLING SS



5
57270
3
NUT, 5/16-18 CAPTIVE "J" PLTD



6
62811
1
PLATE, SQG RETAINER TOP



7
62812
8
PLATE, SQUEEGEE FILLER



8
62813
7
PLATE, SQG BLADE RETAINER



9
66276
2
PIN, CLEVIS 5/16 X 1.625 LG



10
67380
4
RIVET, 5/32 OF X 1/8 GRIP



11
70105
2
SCR, 1/4-20 X 1.75 HHCS   PLTD



12
70291
2
SCR, 1/4-20 X 1.5 ELEVATOR



13
70377
2
SCR, 3/8-16 X 1.25 HHCS GR5PLT



14
70385
2
SCR, 3/8-16 X 2.0 HHCS GR5 PLT



15
70678
2
SCR, 3/8-16X3.5 CARRIAGE PLTD



16
70679
2
SCR, 3/8-16 X 2.5 TAP



17
70680
3
SCR, 5/16-18X1 THUMB SS TYPE P



18
73576
2
SPRING, COMP .60D X2.0L X.045W



19A
73900
1
SQGE BLADE, REAR LINATEX 44"

(STANDARD)

19B
73902
-
SQGE BLADE, REAR (TILE) 44"

(OPTION)

19C
73901
-
SQGE BLADE, REAR (BUTTONS) 44"

(OPTION)

20
78034
1
TUBE, 1.5 OD X 2.5 VAC INTAKE



21
80605
2
COTTER, 5/16" RING



22
81488
1
LATCH, SQUEEGEE STRAP



23
81489
1
STRIKER, SQUEEGEE STRAP REAR



24
81535
4
KNOB, 3/8-16 4 PRONG



25A
82528
1
SQUEEGEE, FRONT BLADE LINATEX

(STANDARD)

25B
82637
-
SQUEEGEE, FRONT BLADE (TILE)

(OPTION)

25C
82640
-
SQUEEGEE, FRONT BLADE (BUTTON)

(OPTION)

26
87030
2
WASHER, 3/8 ID X 3/4 OD NYLON



27
89059
2
WHEEL, BUMPER



28
89197
2
WHEEL, 2 OD X.31IDX.875W, GRY



29
140380
1
BAND, SQUEEGEE FRONT



30
140381
1
BAND, SQUEEGEE REAR



31
140382
1
BAND, SQUEEGEE REAR (S)



32
140385
2
BRKT, WHEEL MOUNT
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REF
PART NO.
QTY
DESCRIPTION
SERIAL NO.

FROM
NOTES:

1
27794
1
CABLE, 23.70 X 1/8



2
36133
1
GRIP, 3/16 X 1.0 FLAT BAR



3
51289
1
LEVER, SQUEEGEE LIFT



4
51322
1
LINKAGE, SQUEEGEE LIFT



5
51323
1
LINKAGE, SQUEEGEE PIVOT



6
57006
1
NUT, 1/4-20 HEX



7
57047
3
NUT, 1/4-20 HEX NYLOCK



8
57113
1
NUT, 5/16-18 HEX NYLOCK



9
57119
1
NUT, 3/8-16 HEX NYLOCK



10
57153
1
NUT, 1/2-13 X HEX NYLOCK THIN



11
64096
1
PULLEY, 1.5 OD X .5 W X .25 B



12
66191
1
PIN, CLEVIS 3/16” X 1/2” PLTD



13
67423
1
RAIL RACHET



14
70297
1
SCR, 1/4-20 X 1.5 HHMS



15
70641
1
SHOULDER BOLT, 3/8OD X 3/8L SS



16
70341
1
SCR, 1/2-13 X 2.5 HHCS GR5PLT



17
70685
1
SCR, 3/8-16 X2.75 HHTB GR5 PLTD



18
730006
1
SPRING, COMP 1.100DX2.0LX.148W



19
73265
2
SPRING, .80D X 4.00L X .120W
1000037808
WAS 73979 (BSS432)

20
78430
3
TUBE, .38 OD X .26 ID X .38 LG



21
80604
2
COTTER, 1/4 RING



22
80606
1
COTTER, 3/8 RING



23
80607
1
COTTER, 1/2 RING



24
80612
1
PIN, CLEVIS 1/4 X 1.0



25
48077
1
KNOB, 3.50 ODX3/8-16 THRU HOLE



26
82060
1
PIN, CLEVIS 3/8 X 5.25



27
82322
1
PIN, CLEVIS 1/2 X 4.80



28
87086
1
WASHER, M10 X 30 PLTD



29
87030
2
WASHER, 3/8 ID X 3/4 OD NYLON



30
87056
1
WASHER, M6 FLAT



31
87135
4
WASHER, .26 ID X .50 OD



32
87200
3
WASHER, .4 ID X 1.3 OD NYLON



33
87201
2
WASHER, 0.781 ID FIBERGLIDE



34
140293
1
SPACER, .75 OD X .50 ID X 1.50 L



35
140379
1
BRACKET, SQUEEGEE MOUNT



36
80815
2
BEARING, FLANGED PLASTIC



37
80582
1
CHAIN, #1/0 7-LINKS GROUNDING



38
73831
1
S-HOOK, 2"
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REF
PART NO.
QTY
DESCRIPTION
SERIAL NO.

FROM
NOTES:

1
34337
1
FILTER, 24 VAC



2
35122
1
GASKET, 230V VAC MOTOR    



3
35211
1
GASKET, 8.50 X 16.40 X .50T



4
35212
1
GASKET, 6.30 X 16.1 C .50T



5
35214
1
GASKET, VAC MOTOR



6
39547
1
HOSE ASM, 1.5 BLK VAC X 21



7
53631
1
VAC MOTOR ASM, 24VDC 3 STAGE




14548
-
BRUSH SET, 24VDC 5.7 3ST VCMTR

(NOT SHOWN)

8
57104
4
NUT, 10-32 W/STAR WASHER PLTD



9
57245
3
NUT, 1/4-20 HEX NYLOCK SS



10
62805
1
PLATE, VAC MOUNT         



11
70607
4
SET SCR, #10-32 X 1.00 SS          



12
70638
3
SCR, 1/4-20 X 1.75 SSSCU       



13
73566
3
SPACER, 1/2 OD X 3.0 W/1/4-20 AL      



14
87013
3
WASHER, 1/4 ID X 5/8 OD SS    
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REF
PART NO.
QTY
DESCRIPTION
SERIAL NO.

FROM
NOTES:

1
05128
1
AXLE, MOTOR DRIVE 24 VDC



2
18041
2
CASTER, 4” DIA. X 2 X 3.56 R



3
57113
4
NUT, 5/16-18 HEX NYLCK



4
57119
8
NUT, 3/8-16 HEX NYLOCK



5
57128
8
NUT, 5/16-24 HEX NYLOCK



6
62714
2
PLATE, DRIVE AXLE



7
70266
8
SCR, 3/8-16 X 1.00 HHCS GR5



8
70325
4
SCR, 5/16-18 X 1.25 HHCS GR5



9
87003
8
WASHER, 3/8 X 7/8 FLAT SS



10
87029
4
WASHER, 5/16 FLAT SS



11A
89155
2
WHEEL, 10” PNEU. NON-MARKING

(STANDARD)


78414
-
TUBE, 10” TIRE

(NOT SHOWN)

11B
89175
-
WHEEL ASY, 10IN PNEU, BLACK

(OPTION)


78414
-
TUBE, 10” TIRE

(NOT SHOWN)

11C
830748
-
WHEEL ASM, 10” SOLID SPCL  SCBR



11D
89211
-
WHEEL ASM, 10” FMFL N-MARKING



11E
89212
-
WHEEL ASM, 10” FMFL BLK KNOBBY



12
89190
1
WELDMENT, FRAME
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REF
PART NO.
QTY
DESCRIPTION
SERIAL NO.

FROM
NOTES:

1
23125
3
WIRE, 4 X 15 B CLAMP



2
23190
1
CABLE, 4 X 27 RED



3
23191
1
CABLE, 4 X 27 BLK



4
70010
2
SCR, 1/4-20 X 1.5 HHCS      SS



5
82803
2
CONNECTOR, RED 24V



6
87025
2
WASHER, 1/4 LOCK EXT STAR  SS



7
81366
2
CABLE, ELECTRICAL 4GA X 82.5



8
880209
1
WIRE ASM, CHARGER ADAPTER 24V



9
70114
1
SCR, #10 X 3/4 PPHST TYPE B



10
20054
2
CLAMP, 3/8 NYLON UL/CSA
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