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Bulletin # 0004000





December 23, 2002











Betco Part #86647 40-amp fuse.





Serial numbers beginning BC02D-BC02F 





Motor spike may cause 30-amp fuse to fail, replace with 40-amp fuse.
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Service Managers:





This is to notify you of a potential part failure on our Watchman 20 & 24 Automatic Scrubbers.  A 30-amp fuse that controls power to the vacuum motor has failed in certain instances. Not all machines are experiencing this fuse failure, however if you do receive one of these machines in for service it is recommended that you replace the 30-amp fuse with a 40-amp fuse. Please see the below diagram for details. 























Replace 30-amp fuse (3rd from left) with a 40-amp fuse.

















To: 		Authorized Betco Service Centers





From: 	Chris Keene - Equipment Marketing Manager





Subject: 	Watchman 20 & 24 Automatic Scrubber – Potential Fuse Failure
































