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Service Managers:


This is to notify you of a potential service requirement on Betco burnisher models 83004 Foreman 1600 and 83005 Foreman 2000. In some instances the trigger assembly may not make solid contact with the safety switch plunger. If you receive one of these units experiencing this problem, order and install this kit.





Replacement Kit Instructions (Also included with the kit)


Unplug the power cord of the machine.


Remove the 4 Phillips head screws on the rear of the switchbox using a # 3 Phillips screwdriver.


Remove the existing trigger, discard and replace with the new trigger (note that it has a slightly longer protrusion that contacts the switch).


Remove the Phillips screws in the switch (use a # 2 Screwdriver) and add the plate as shown.


Replace the back cover.


Test, the switch should not operate unless the safety switch is actuated to allow movement of the trigger.





Caution: When replacing the trigger, it must only be used with the supplied plate. Failure to install the plate could cause the safety switch to become ineffective causing injury if the machine is turned on accidentally.





Betco Order Number: 83128-00


Unit: 1 Each


Description: Trigger switch and plate kit


MSRP: $ 9.72


Distributor Cost: $ 5.83














Should you have any questions please contact 


our Technical Support Team:
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To: 		Authorized Betco Service Centers





From: 	Chris Keene – Category Manager





Subject: 	Foreman( 1600 and Foreman( 2000 Burnisher 


Trigger and Switch Plate Replacement Kit 
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