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�CREWMAN™ 2000DC Dust Control Burnisher








�





Product Applications:


Hard floor�
Burnishing�
�






Product Listing:


E83018-00�
CREWMAN™ DC2000 Dust Control Burnisher�
�






Description:  The CREWMAN™ 2000DC combines the power of 2000 RPM’s with precision balancing and advanced dust control to deliver superior high speed burnishing results. A unique spring loaded motor design provides maximum pad to floor contact and an even burnish every time!





Market Segments:  The healthcare market is a key area of opportunity. The passive dust control system effectively captures dust and contains it in an onboard cloth bag.





Positioning:  Highly responsive burnish results are achieved with this durable and dependable dust control burnisher. A low price and the support of our 10/3 warranty make it an industry BEST VALUE !





Benefit to Distributor:  Crewman™ burnishers will compliment your existing equipment line by meeting the growing need for “”competitively priced” products without sacrificing product quality. 





Steps for the Distributor Sales Professional: 


Review the product with your Betco Regional Manager.


Identify target end-users and perform qualified demonstrations.














