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Sales and Service Managers:





This bulletin is to notify you of the differences between the bristle pad driver that comes standard with each unit and the optional bristle stripping brush available. Please review the below information.








































































































To: 		Authorized Betco Equipment Distributors


From: 	Chris Keene – Category Manager


Subject: 	Toughman( Propane and Battery Strip Machines


	Pad Driver vs. Strip Brush 





Each Toughman™ strip machine comes standard with a bristle pad driver as shown in figure 1. The bristle construction of the pad driver allows emulsified floor coatings to migrate completely through the floor pad and up through the pad driver. This provides a more consistent scrubbing action and prevents build up within the stripping pad.





Note – DO NOT use the pad driver as a brush. This can cause damage to the machine, pad driver and the floor.
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Figure 2. 
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August 15, 2003





Betco does offer an optional stripping brush for the Toughman™ strip machines, as shown in figure 2. Highly aggressive, this brush is ideal for applications where heavy duty stripping and soil removal is required.





Betco Order Number: 82018-00


Unit: 1 Each


Description: Strip Brush for Toughman Machines
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Figure 1.
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