**Hako Updater**

1. Download all files in Diag Updates

2. Put all files into one folder on your desktop.

3. Run the HakoDiagnose MainSetup2020.exe

4. Install this program at the end it will restart your computer.

5. When your computer is rebooted you will see a new icon on your desktop called Hako Diagnose

6. Go back to your folder you created and run the updates in order from 1-4

7. You will not have to restart after each update.

8. Once all updates are complete go to your desktop and right click on Hako Diagnose.

9. Select Properties > Open File Location

10. From the folder you have created copy and move the LicKey.hli from your folder to the folder created by Hako Diagnose. The file extension will look something like C:\MDT\Hako

11. Once this is complete your Hako Diagnose is up to Date.

12. Follow Hako instructions to update your unit.

13. To update software, select the unit CAN FLASHER tab for the unit you have (B120R or B175R)

14. On the next screen, select “Flash Software”

15. On the next screen you’ll notice the current software version. Click OK below to load and update the software with the new.

16. Once done, you can go through the same sequence to verify the software version has changed. If so, turn the unit off. Unplug the cables and test the unit